**HYGIENE+ waste**

Chrome-plated brass concave grid

Reference: **AT611**

Specification description

Hygienic washbasin waste M1 1/4" with concave grid (no water retention).

Free flow, with no central screw (avoids scale deposits and reduces bacterial development).

Polished chrome-plated brass grid, chrome-plated ABS body.

Can be tightened to a minimum of 1mm or maximum of 45mm.

Pre-scored waste: snap-off sections can be removed for models with overflow.

Complies with European standard EN 274-1.